{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"merged":[[0,0,0,5],[11,0,11,5],[21,0,21,5],[31,0,31,5]],"flags":["formulas_cached_only"]}
["主 干 管 线 传 输 系 统"]
["序号","设备名称","品牌","技术指标","数量","单位"]
[1,"超5类网线","安普","UTP超5类4对非屏蔽电缆，国标",800,"米"]
[2,"6类网线","安普","UTP六类4对非屏蔽电缆；国标",1200,"米"]
[3,"电缆","九州","国产 RVV2×4.0（纯铜）户外防水",1500,"米"]
[4,"电缆","九州","国产 RVV2×1.0（纯铜）户外防水",500,"米"]
[5,"光纤","九州","光缆室外地埋铺设",1000,"米"]
[6,"光纤配设","室外","含法兰、光配架、尾纤、跳线、熔接费用等",16,"个"]
[7,"PVC管材",null,"抗充耐热、阻燃、耐腐蚀、防虫、绝缘性能好",2000,"米"]
[8,"切路","回填含管","切割路面",40,"米"]
[9,"辅材","采购","安装工具，缠绕管，扎带，胶带，膨胀螺丝、水晶头等",1,"批"]
["前 端 视 频 设 备"]
[1,"红外高清网络枪型摄像机","大华","1、具有200W像素 CMOS传感器。  \n2、在1920x1080 @25fps下，码率设定为1Mbps，RJ45输出，清晰度不小于1000TVL。  \n*3、支持滤光片切换功能，摄像机可在彩色/黑白模式下自动切换滤光片。 \n4、最低照度彩色：0.001lx，黑白：0.0005 lx。\n5、支持H.265、H.264、MJPEG视频编码格式，其中H.265和H.264都支持Baseline/Main/High Profile                                      6、支持五码流技术，五码流可同时输出，主码流最大1920x1080@30fps，第二码流最大704x480@30fps，第三码流最大1920x1080 @30fps，第四码流最大704x480@30fps，第五码流最大1920x1080@30fps。\n",34,"台"]
[2,"红外高清星光级摄像机","大华","1、具有400W像素 CMOS传感器。  \n2、在1920x1080 @25fps下，码率设定为1Mbps，RJ45输出，清晰度不小于1000TVL。  \n*3、支持滤光片切换功能，摄像机可在彩色/黑白模式下自动切换滤光片。 \n4、最低照度彩色：0.001lx，黑白：0.0005 lx。\n5、支持H.265、H.264、MJPEG视频编码格式，其中H.265和H.264都支持Baseline/Main/High Profile                                      6、支持五码流技术，五码流可同时输出，主码流最大1920x1080@30fps，第二码流最大704x480@30fps，第三码流最大1920x1080 @30fps，第四码流最大704x480@30fps，第五码流最大1920x1080@30fps。\n",20,"台"]
[3,"红外高清网络球型摄像机","DS-2DC","1、1/2.8英寸 CMOS,200W像素  \n2、23倍光学变倍，16倍数字变倍\n3、支持H.265编码，实现超低码流传输 \n4、支持水平手控速度最大为670°/S，云台定位精度为±0.1°  \n5、分辨力不小于1100TVL（分辨力为1920*1080，帧率为60fps/S）   \n6、支持输出图像失真小于等于2.5%  \n7、支持宽动态不低于105.6dB，且综合得分116分  \n8、设备应不少于1000个预置位 \n9、内置150米红外灯补光，采用倍率与红外灯功率匹配算法，补光效果更均匀  \n10、支持32条巡航路径，每条巡航可以添加32个预置点  \n",2,"台"]
[4,"摄像机支架",null,"尺寸为190.5*88.0*58.0mm，采用铝合金材质，不易生锈，白色",54,"个"]
[5,"摄像机电源","小耳朵","12V 2A，室外防水",54,"个"]
[6,"室外防水设备箱",null,"符合室外防水标准",30,"个"]
[7,"立杆",null,"3.5m，喷塑",4,"根"]
[8,"支架加工",null,"定做",6,"套"]
[9,"辅材","采购","安装工具，缠绕管，扎带，胶带，膨胀螺丝、水晶头等",1,"宗"]
["视 频 传 输 设 备"]
[1,"接入交换机","华为","1.封包缓冲：≥448Kbit ,保证视频不卡顿；2.转发性能：交换延迟<5μs\n3.支持宽压：12VDC-36VDC ；4.低功耗：满载功耗小于3瓦\n\n\n",30,"台"]
[2,"中继器","华为","点对点无线室外大功率千兆商用5公里",16,"台"]
[3,"汇聚交换机","华为","24个10/100/1000Base-T",3,"台"]
[4,"千兆光纤收发器","CDM-1000M","支持10Base-T、 100Base-TX 或1000Base-T自适应与1000Base-SX/LX间相互转换；支持全双工和半双工传输模式，能自动协商；支持双绞线口自动交叉，方便系统调试安装；支持VLAN超长数据包传输；支持QoS，保证VOIP数据包传输；支持STP生成树，构成冗余网络；",6,"对"]
[5,"漏电保护开关","公牛","2P/16A",20,"个"]
[6,"防雷模块","公牛","选用进口优质压敏电阻器，高可靠的质量保证；模块式设计，更换方便；采用温控断路技术，避免火灾发生；通流容量大；响应时间快；残压低；标准35mm导轨安装；安装方便，维护简单。",32,"个"]
[7,"落地式防水设备配电箱","定做","加厚钢板，喷塑，80cm*60cm*40cm",4,"套"]
[8,"插排","公牛","知名品牌",30,"个"]
[9,"辅材",null,"光缆熔接、线槽线管及配件等",1,"宗"]
["主 控 系 统 设 备"]
[1,"网络高清硬盘录像机","大华","1、采用LINUX操作系统，支持电源、风扇、磁盘等模块热插拔，标配8G内存，可扩展不低于32G；具有128G的SSD。\n2、支持H.264、H.265、SVAC、MPEG4、MJPEG视频编码格式，支持G.711a、G.711u、G.726、AAC音频编码格式的IPC接入。\n3、支持SATA、SAS磁盘，支持SSD，支持磁盘混插，支持2.5/3.5英寸磁盘，支持磁盘负载均衡工作，支持Raid功能，支持全局热备和本地热备。\n\n",2,"台"]
[2,"监控级硬盘","希捷","满足2个月存储",8,"块"," "]
[3,"VGA数据线","联想","符合国标",2,"条"]
[4,"键盘鼠标","联想","光电套装，防水，耐磨，按键灵活",2,"套"]
[5,"网络机柜","图腾","静载承重不小于1000KG（带支架）；防护等级:IP20。",1,"台"]
[6,"操作台","跃达","三联操作台",1,"套"]
[7,"监视器",null,"42英寸 监视器 宽屏LED",2,"台"]
[8,"辅材",null,"光缆熔接、线槽线管及配件等",1,"宗"]